Each {ANYNODE} operates independently as a self-contained universal computing unit. However, in scenarios like edge clusters, data centers, or private clouds, containers or VMs may require seamless, high-performance local network connectivity across nodes. Sky Network, also known as Global Private Layer 2 Network (GPL2N), addresses this need with a low-latency, high-throughput mesh networking layer built into the Sky Router system. While both Sky Network and Sky Link use encrypted point-to-point tunnels, Sky Link connects {ANYNODE}s over wide-area networks, whereas Sky Network is designed to extend Layer 2 connectivity locally across nodes. It enables transparent guest network extension, supports DHCP and broadcast traffic, and avoids the complexity of traditional SDN or VXLAN overlays. This provides a unified LAN-like environment across distributed nodes, simplifying deployment and ensuring consistent, responsive performance.
Important
For optimal performance, the response time between Sky Nodes connected to a Sky Network should not exceed 45 milliseconds.