A private network defines an IP range within the scope of a {ANYNODE} and is used to create networks on which containers and virtual machines can connect. By default, a node includes two networks: xcNET (Managed Network) and xcLAN (DLAN/VLAN Network). When a {NEBULA} system is deployed, its private network xcNET is set to {DEFCNIP}.N.0.0/16, where N represents the IPN (IP Order Number) of the node. Each {NEBULA} deployment increments the IPN, with a maximum of 250 IPNs allowed for an Admin account. The default xcLAN is a DLAN (Direct LAN) network that contacts the DHCP server of the {ANYNODE}'s primary IP network range to receive a LAN IP address. This configuration places the container or virtual machine within the same network as the {ANYNODE}.