The create command provisions a new network on a {ANYNODE}.
JSON Input Data Format

    {
        "cloudid": string,
        "name": string,
        "nettype": string,
        "network": string,
        "mask": string
    }

cloudid * | Specifies the ID of the {ANYNODE} on which the network will be created.
name * | Specifies the name for the network. Input rules require that no spaces are allowed.
nettype * | Specifies the network type which includes: managed Specifies a managed network within the scope of the {ANYNODE} and creates a DHCP server for the network. lan Specifies the creation of a network bridge over an existing network device on the {ANYNODE}.
network * | Specifies the network IP range. The following rules apply: If the nettype is set to "managed": Input the network IP range, such as 16.100.0.0. The network IP range must end with .0. If the nettype is set to "lan": Input the * (asterisk) character.
mask * | Specifies the network mask number. The following rules apply: If the nettype is set to "managed": Enter the network mask, which must be a number between 16 and 30. If the nettype is set to "lan": Input the * (asterisk) character.

* Indicates a mandatory field.

Code Snippets
Here are several code snippets provided for your direct use. Simply select your preferred tool/language by clicking on it.
Successful Response

    {
        "result": "OK",
        "payload": "The process was successfully completed",
        "id": "V7-49ff499f-xxxx-xxxx-xxxx-b47fxxxx99af"
    }

Failed Response

    {
        "result": "ERR",
        "message": "Error message ..."
    }